hda: IBM-DJSA-220, ATA DISK drive
hda: IBM-DJSA-220, ATA DISK drive
hda: IBM-DJSA-220, ATA DISK drive
hda: IBM-DJSA-220, ATA DISK drive
ide0 at 0x000-0x007,0x038 on irq 6
hda: IBM-DJSA-220, 19077MB w/1874kB Cache, CHS=38760/16/63
empeg-flash driver initialized
smc chip id/revision 0x3349
smc9194.c:v0.12 03/06/96 by Erik Stahlman (erik@vt.edu)

SMC9194: SMC91C94(r:9) at 0x4008000 IRQ:7 INTF:TP MEM:6144b MAC 00:02:d7:12:02:8
c
Partition check:
 hda: hda1 < hda5 hda6 > hda2 hda3 hda4
RAMDISK: ext2 filesystem found at block 0
RAMDISK: Loading 320 blocks [1 disk] into ram disk... done.
EXT2-fs warning: checktime reached, running e2fsck is recommended
VFS: Mounted root (ext2 filesystem).
empeg-pump v0.03 (19980601)
Press Ctrl-A to enter pump...hange_root: old root has d_count=1
Trying to unmount old root ... okay
Freeing  player.cpp        : 385:empeg-car 2.00 2003/04/01.
Prolux 4 empeg car - 2.1434 Mar 26 2003
Vcb: 0x4054d000
Player received SIGINT, user interruption
Switching to shell-player loop
Starting bash.
no shell!
Shell exit
  player.cpp        : 385:empeg-car 2.00 2003/04/01.
Prolux 4 empeg car - 2.1434 Mar 26 2003
Vcb: 0x4054d000
ide_data_test: wrote 0x0000 read 0x0001
ide_data_test: wrote 0xffff read 0x0001
ide_data_test: wrote 0xaaaa read 0x0001
ide_data_test: wrote 0x5555 read 0x0001
hda: WDC WD1200BEVE-00UYT0, ATA DISK drive
ide_data_test: wrote 0x0000 read 0x0001
ide_data_test: wrote 0xffff read 0x0001
ide_data_test: wrote 0xaaaa read 0x0001
ide_data_test: wrote 0x5555 read 0x0001
hda: WDC WD1200BEVE-00UYT0, ATA DISK drive
ide_data_test: wrote 0x0000 read 0x0001
ide_data_test: wrote 0xffff read 0x0001
ide_data_test: wrote 0xaaaa read 0x0001
ide_data_test: wrote 0x5555 read 0x0001
hda: WDC WD1200BEVE-00UYT0, ATA DISK drive
ide_data_test: wrote 0x0000 read 0x0001
ide_data_test: wrote 0xffff read 0x0001
ide_data_test: wrote 0xaaaa read 0x0001
ide_data_test: wrote 0x5555 read 0x0001
hda: WDC WD1200BEVE-00UYT0, ATA DISK drive
ide0 at 0x000-0x007,0x038 on irq 6
hda: WDC WD1200BEVE-00UYT0, 114473MB w/8192kB Cache, CHS=14593/255/63
empeg-flash driver initialized
smc chip id/revision 0x3349
smc9194.c:v0.12 03/06/96 by Erik Stahlman (erik@vt.edu)

SMC9194: SMC91C94(r:9) at 0x4008000 IRQ:7 INTF:TP MEM:6144b MAC 00:02:d7:12:02:8
c
Partition check:
 hda: hda1 < hda5 hda6 > hda2 hda3 hda4
RAMDISK: ext2 filesystem found at block 0
RAMDISK: Loading 320 blocks [1 disk] into ram disk... done.
EXT2-fs warning: checktime reached, running e2fsck is recommended
VFS: Mounted root (ext2 filesystem).
empeg-pump v0.03 (19980601)
Press Ctrl-A to enter pump...VFS: Mounted root (ext2 filesystem) readonly.
change_root: old root has d_count=1
Builder image
show_message("Builder image")
Setting up swapspace version 0, size = 16412672 bytes
Adding Swap: 16028k swap-space (priority -1)
Setting up swapspace version 0, size = 24670208 bytes
Adding Swap: 24092k swap-space (priority -2)
Tuning hda5
show_message("Tuning hda5")
tune2fs 1.17, 26-Oct-1999 for EXT2 FS 0.5b, 95/08/09
Setting maximal mount count to -1
Setting interval between check 0 seconds
Making hda4 filesystem
show_message("Making hda4 filesystem")
mke2fs 1.14, 9-Jan-1999 for EXT2 FS 0.5b, 95/08/09
ext2fs_check_if_mount: No such file or directory while determining whether /dev/
hda4 is mounted.
Linux ext2 filesystem format
Filesystem label=
457728 inodes, 29278462 blocks
0 blocks (0.00%) reserved for the super user
First data block=0
Block size=4096 (log=2)
Fragment size=4096 (log=2)
894 block groups
32768 blocks per group, 32768 fragments per group
512 inodes per group
Superblock backups stored on blocks:
        32768, 98304, 163840, 229376, 294912, 819200, 884736, 1605632, 2654208,

        4096000, 7962624, 11239424, 20480000, 23887872,

Writing inode tables: done
Writing superblocks and filesystem accounting information: done
Tuning hda4
show_message("Tuning hda4")
tune2fs 1.17, 26-Oct-1999 for EXT2 FS 0.5b, 95/08/09
Setting maximal mount count to -1
Setting interval between check 0 seconds
Mounting hda4
show_message("Mounting hda4")
Making directories
show_message("Making directories")
Remounting ro
show_message("Remounting ro")
hda4 completed
show_message("hda4 completed")
Zeroing hda3
show_message("Zeroing hda3")
/bin/cat: write error: No space left on device
Done!
show_message("Done!")
bash-2.01#

empeg-car bootstrap v1.00 20000601 (hugo@empeg.com)
If there is anyone present who wants to upgrade the flash, let them speak now,
or forever hold their peace...it seems not. Let fly the Penguins of Linux!

e000 v1.04
Copying kernel...
Calling linux kernel...
Uncompressing Linux..................................... done, booting the kerne
l.
Linux version 2.2.17-rmk5-np17-empeg55-hijack-v508 (hijack@rtr.ca) (gcc version
2.95.3 20010315 (release)) #2 Fri Jan 9 16:06:35 EST 2009
Processor: Intel StrongARM-1100 revision 11
Checking for extra DRAM:
c0c00000: wrote ffffffff, read e28cc001
NetWinder Floating Point Emulator V0.94.1 (c) 1998 Corel Computer Corp.
empeg-car player (hardware revision 7, serial number 90000652) 12MB DRAM
Command line: mem=12m
Calibrating delay loop... 207.67 BogoMIPS
Memory: 10944k/12M available (996k code, 20k reserved, 324k data, 4k init)
Dentry hash table entries: 2048 (order 2, 16k)
Buffer cache hash table entries: 16384 (order 4, 64k)
Page cache hash table entries: 4096 (order 2, 16k)
POSIX conformance testing by UNIFIX
Linux NET4.0 for Linux 2.2
Based upon Swansea University Computer Society NET3.039
NET4: Linux TCP/IP 1.0 for NET4.0
IP Protocols: ICMP, UDP, TCP
TCP: Hash tables configured (ehash 16384 bhash 16384)
IrDA (tm) Protocols for Linux-2.2 (Dag Brattli)
Starting kswapd v 1.5
SA1100 serial driver version 4.27 with no serial options enabled
ttyS00 at 0xf8010000 (irq = 15) is a SA1100 UART
ttyS01 at 0xf8050000 (irq = 17) is a SA1100 UART
ttyS02 at 0xf8030000 (irq = 16) is a SA1100 UART
Signature is ffffffff 'ÿÿÿÿ'
Tuner: loopback=0, ID=-1
show_message("Hijack v508 by Mark Lord")
empeg display initialised.
empeg dsp audio initialised
empeg dsp mixer initialised
empeg dsp initialised
empeg audio-in initialised, CS4231A revision a0
empeg remote control/panel button initialised.
empeg usb initialised, PDIUSBD12 id 1012
empeg state support initialised 0089/88c1 (save to d0004280).
empeg RDS driver initialised
empeg power-pic driver initialised (first boot)
RAM disk driver initialized:  16 RAM disks of 4096K size
empeg single channel IDE
Probing primary interface...
ide_data_test: wrote 0x0000 read 0x8080
ide_data_test: wrote 0xffff read 0x8080
ide_data_test: wrote 0xaaaa read 0x8080
ide_data_test: wrote 0x5555 read 0x8080
ide_data_test: wrote 0x0000 read 0x8080
ide_data_test: wrote 0xffff read 0x8080
ide_data_test: wrote 0xaaaa read 0x8080
ide_data_test: wrote 0x5555 read 0x8080
ide_data_test: wrote 0x0000 read 0x8080
ide_data_test: wrote 0xffff read 0x8080
ide_data_test: wrote 0xaaaa read 0x8080
ide_data_test: wrote 0x5555 read 0x8080
ide_data_test: wrote 0x0000 read 0x8080
ide_data_test: wrote 0xffff read 0x8080
ide_data_test: wrote 0xaaaa read 0x8080
ide_data_test: wrote 0x5555 read 0x8080
ide_data_test: wrote 0x0000 read 0x0000
ide_data_test: wrote 0xffff read 0xffff
ide_data_test: wrote 0xaaaa read 0xaaaa
ide_data_test: wrote 0x5555 read 0x5555
hda: IBM-DJSA-220, ATA DISK drive
hdb: WDC WD1200BEVE-00UYT0, ATA DISK drive
ide0 at 0x000-0x007,0x038 on irq 6
hda: IBM-DJSA-220, 19077MB w/1874kB Cache, CHS=38760/16/63
hdb: WDC WD1200BEVE-00UYT0, 114473MB w/8192kB Cache, CHS=14593/255/63
empeg-flash driver initialized
smc chip id/revision 0x3349
smc9194.c:v0.12 03/06/96 by Erik Stahlman (erik@vt.edu)

SMC9194: SMC91C94(r:9) at 0x4008000 IRQ:7 INTF:TP MEM:6144b MAC 00:02:d7:12:02:8
c
Partition check:
 hda: hda1 < hda5 hda6 > hda2 hda3 hda4
 hdb: hdb1 < hdb5 hdb6 > hdb2 hdb3 hdb4
RAMDISK: ext2 filesystem found at block 0
RAMDISK: Loading 320 blocks [1 disk] into ram disk... done.
EXT2-fs warning: checktime reached, running e2fsck is recommended
VFS: Mounted root (ext2 filesystem).
empeg-pump v0.03 (19980601)
empeg-pump v0.03 (19980601)
change_root: old root has d_count=1
Trying to unmount old root ... okay
Freeing unused kernel memory: 4k initempeg init 0.8
I see this is a developer image!
Mounting proc
Mounting first music partition
Tried to mount /dev/hda4 as reiserfs but got error 19
Mounting second music partition
Remounting first music partition read-only
Remounting second music partition read-only
Press 'q' now to go into development mode. You Have Zero Seconds To Comply...
Starting player
Timezone: NZ-CHAT
Hijack: intercepting config.ini

hijack: removed menu entry: "Hard Disk Detection"
hijack: removed menu entry: "Serial Port Assignment"
kftpd: listening on port 21
khttpd: listening on port 80
  player.cpp        : 385:empeg-car 2.01 2004/07/06.
Prolux 4 empeg car - 2.1434 Jul  5 2004
Vcb: 0x40577000
! wave_decoder.cpp  : 312:Bytes not (yet) available (0xc0044000)

empeg-car bootstrap v1.00 20000601 (hugo@empeg.com)
If there is anyone present who wants to upgrade the flash, let them speak now,
or forever hold their peace...it seems not. Let fly the Penguins of Linux!

e000 v1.04
Copying kernel...
Calling linux kernel...
Uncompressing Linux..................................... done, booting the kerne
l.
Linux version 2.2.17-rmk5-np17-empeg55-hijack-v508 (hijack@rtr.ca) (gcc version
2.95.3 20010315 (release)) #2 Fri Jan 9 16:06:35 EST 2009
Processor: Intel StrongARM-1100 revision 11
Checking for extra DRAM:
c0c00000: wrote ffffffff, read e28cc001
NetWinder Floating Point Emulator V0.94.1 (c) 1998 Corel Computer Corp.
empeg-car player (hardware revision 7, serial number 90000652) 12MB DRAM
Command line: mem=12m
Calibrating delay loop... 207.67 BogoMIPS
Memory: 10944k/12M available (996k code, 20k reserved, 324k data, 4k init)
Dentry hash table entries: 2048 (order 2, 16k)
Buffer cache hash table entries: 16384 (order 4, 64k)
Page cache hash table entries: 4096 (order 2, 16k)
POSIX conformance testing by UNIFIX
Linux NET4.0 for Linux 2.2
Based upon Swansea University Computer Society NET3.039
NET4: Linux TCP/IP 1.0 for NET4.0
IP Protocols: ICMP, UDP, TCP
TCP: Hash tables configured (ehash 16384 bhash 16384)
IrDA (tm) Protocols for Linux-2.2 (Dag Brattli)
Starting kswapd v 1.5
SA1100 serial driver version 4.27 with no serial options enabled
ttyS00 at 0xf8010000 (irq = 15) is a SA1100 UART
ttyS01 at 0xf8050000 (irq = 17) is a SA1100 UART
ttyS02 at 0xf8030000 (irq = 16) is a SA1100 UART
Signature is ffffffff 'ÿÿÿÿ'
Tuner: loopback=0, ID=-1
show_message("Hijack v508 by Mark Lord")
empeg display initialised.
empeg dsp audio initialised
empeg dsp mixer initialised
empeg dsp initialised
empeg audio-in initialised, CS4231A revision a0
empeg remote control/panel button initialised.
empeg usb initialised, PDIUSBD12 id 1012
empeg state support initialised 0089/88c1 (save to d0004380).
empeg RDS driver initialised
empeg power-pic driver initialised (first boot)
RAM disk driver initialized:  16 RAM disks of 4096K size
empeg single channel IDE
Probing primary interface...
ide_data_test: wrote 0x0000 read 0x8080
ide_data_test: wrote 0xffff read 0x8080
ide_data_test: wrote 0xaaaa read 0x8080
ide_data_test: wrote 0x5555 read 0x8080
ide_data_test: wrote 0x0000 read 0x8080
ide_data_test: wrote 0xffff read 0x8080
ide_data_test: wrote 0xaaaa read 0x8080
ide_data_test: wrote 0x5555 read 0x8080
ide_data_test: wrote 0x0000 read 0x8080
ide_data_test: wrote 0xffff read 0x8080
ide_data_test: wrote 0xaaaa read 0x8080
ide_data_test: wrote 0x5555 read 0x8080
ide_data_test: wrote 0x0000 read 0x8080
ide_data_test: wrote 0xffff read 0x8080
ide_data_test: wrote 0xaaaa read 0x8080
ide_data_test: wrote 0x5555 read 0x8080
ide_data_test: wrote 0x0000 read 0x0000
ide_data_test: wrote 0xffff read 0xffff
ide_data_test: wrote 0xaaaa read 0xaaaa
ide_data_test: wrote 0x5555 read 0x5555
hda: IBM-DJSA-220, ATA DISK drive
hdb: WDC WD1200BEVE-00UYT0, ATA DISK drive
ide0 at 0x000-0x007,0x038 on irq 6
hda: IBM-DJSA-220, 19077MB w/1874kB Cache, CHS=38760/16/63
hdb: WDC WD1200BEVE-00UYT0, 114473MB w/8192kB Cache, CHS=14593/255/63
empeg-flash driver initialized
smc chip id/revision 0x3349
smc9194.c:v0.12 03/06/96 by Erik Stahlman (erik@vt.edu)

SMC9194: SMC91C94(r:9) at 0x4008000 IRQ:7 INTF:TP MEM:6144b MAC 00:02:d7:12:02:8
c
Partition check:
 hda: hda1 < hda5 hda6 > hda2 hda3 hda4
 hdb: hdb1 < hdb5 hdb6 > hdb2 hdb3 hdb4
RAMDISK: ext2 filesystem found at block 0
RAMDISK: Loading 320 blocks [1 disk] into ram disk... done.
EXT2-fs warning: checktime reached, running e2fsck is recommended
VFS: Mounted root (ext2 filesystem).
empeg-pump v0.03 (19980601)
Press Ctrl-A to enter pump...VFS: Mounted root (ext2 filesystem) readonly.
change_root: old root has d_count=1
Trying to unmount old root ... okay
Freeing unused kernel memory: 4k initempeg init 0.8
I see this is a developer image!
Mounting proc
Mounting first music partition
Tried to mount /dev/hda4 as reiserfs but got error 19
Mounting second music partition
Remounting first music partition read-only
Remounting second music partition read-only
Press 'q' now to go into development mode. You Have Zero Seconds To Comply...
Starting player
Timezone: NZ-CHAT
Hijack: intercepting config.ini

hijack: removed menu entry: "Hard Disk Detection"
hijack: removed menu entry: "Serial Port Assignment"
kftpd: listening on port 21
khttpd: listening on port 80
  player.cpp        : 385:empeg-car 2.01 2004/07/06.
Prolux 4 empeg car - 2.1434 Jul  5 2004
Vcb: 0x40577000
! wave_decoder.cpp  : 312:Bytes not (yet) available (0xc0044000)

empeg-car bootstrap v1.00 20000601 (hugo@empeg.com)
If there is anyone present who wants to upgrade the flash, let them speak now,
or forever hold their peace...it seems not. Let fly the Penguins of Linux!

e000 v1.04
Copying kernel...
Calling linux kernel...
Uncompressing Linux..................................... done, booting the kerne
l.
Linux version 2.2.17-rmk5-np17-empeg55-hijack-v508 (hijack@rtr.ca) (gcc version
2.95.3 20010315 (release)) #2 Fri Jan 9 16:06:35 EST 2009
Processor: Intel StrongARM-1100 revision 11
Checking for extra DRAM:
c0c00000: wrote ffffffff, read e28cc001
NetWinder Floating Point Emulator V0.94.1 (c) 1998 Corel Computer Corp.
empeg-car player (hardware revision 7, serial number 90000652) 12MB DRAM
Command line: mem=12m
Calibrating delay loop... 207.67 BogoMIPS
Memory: 10944k/12M available (996k code, 20k reserved, 324k data, 4k init)
Dentry hash table entries: 2048 (order 2, 16k)
Buffer cache hash table entries: 16384 (order 4, 64k)
Page cache hash table entries: 4096 (order 2, 16k)
POSIX conformance testing by UNIFIX
Linux NET4.0 for Linux 2.2
Based upon Swansea University Computer Society NET3.039
NET4: Linux TCP/IP 1.0 for NET4.0
IP Protocols: ICMP, UDP, TCP
TCP: Hash tables configured (ehash 16384 bhash 16384)
IrDA (tm) Protocols for Linux-2.2 (Dag Brattli)
Starting kswapd v 1.5
SA1100 serial driver version 4.27 with no serial options enabled
ttyS00 at 0xf8010000 (irq = 15) is a SA1100 UART
ttyS01 at 0xf8050000 (irq = 17) is a SA1100 UART
ttyS02 at 0xf8030000 (irq = 16) is a SA1100 UART
Signature is ffffffff 'ÿÿÿÿ'
Tuner: loopback=1, ID=-1
show_message("Hijack v508 by Mark Lord")
empeg display initialised.
empeg dsp audio initialised
empeg dsp mixer initialised
empeg dsp initialised
empeg audio-in initialised, CS4231A revision a0
empeg remote control/panel button initialised.
empeg usb initialised, PDIUSBD12 id 1012
empeg state support initialised 0089/88c1 (save to d0004480).
empeg RDS driver initialised
empeg power-pic driver initialised (first boot)
RAM disk driver initialized:  16 RAM disks of 4096K size
empeg single channel IDE
Probing primary interface...
ide_data_test: wrote 0x0000 read 0x8080
ide_data_test: wrote 0xffff read 0x8080
ide_data_test: wrote 0xaaaa read 0x8080
ide_data_test: wrote 0x5555 read 0x8080
ide_data_test: wrote 0x0000 read 0x8080
ide_data_test: wrote 0xffff read 0x8080
ide_data_test: wrote 0xaaaa read 0x8080
ide_data_test: wrote 0x5555 read 0x8080
ide_data_test: wrote 0x0000 read 0x8080
ide_data_test: wrote 0xffff read 0x8080
ide_data_test: wrote 0xaaaa read 0x8080
ide_data_test: wrote 0x5555 read 0x8080
ide_data_test: wrote 0x0000 read 0x8080
ide_data_test: wrote 0xffff read 0x8080
ide_data_test: wrote 0xaaaa read 0x8080
ide_data_test: wrote 0x5555 read 0x8080
ide_data_test: wrote 0x0000 read 0x0000
ide_data_test: wrote 0xffff read 0xffff
ide_data_test: wrote 0xaaaa read 0xaaaa
ide_data_test: wrote 0x5555 read 0x5555
hda: IBM-DJSA-220, ATA DISK drive
hdb: WDC WD1200BEVE-00UYT0, ATA DISK drive
ide0 at 0x000-0x007,0x038 on irq 6
hda: IBM-DJSA-220, 19077MB w/1874kB Cache, CHS=38760/16/63
hdb: WDC WD1200BEVE-00UYT0, 114473MB w/8192kB Cache, CHS=14593/255/63
empeg-flash driver initialized
smc chip id/revision 0x3349
smc9194.c:v0.12 03/06/96 by Erik Stahlman (erik@vt.edu)

SMC9194: SMC91C94(r:9) at 0x4008000 IRQ:7 INTF:TP MEM:6144b MAC 00:02:d7:12:02:8
c
Partition check:
 hda: hda1 < hda5 hda6 > hda2 hda3 hda4
 hdb: hdb1 < hdb5 hdb6 > hdb2 hdb3 hdb4
RAMDISK: ext2 filesystem found at block 0
RAMDISK: Loading 320 blocks [1 disk] into ram disk... done.
EXT2-fs warning: checktime reached, running e2fsck is recommended
VFS: Mounted root (ext2 filesystem).
empeg-pump v0.03 (19980601)
Press Ctrl-A to enter pump...VFS: Mounted root (ext2 filesystem) readonly.
change_root: old root has d_countempeg init 0.8
I see this is a developer image!
Mounting proc
Mounting first music partition
Tried to mount /dev/hda4 as reiserfs but got error 19
Mounting second music partition
Remounting first music partition read-only
Remounting second music partition read-only
Press 'q' now to go into development mode. You Have Zero Seconds To Comply...
Starting player
Timezone: NZ-CHAT
Hijack: intercepting config.ini

hijack: removed menu entry: "Hard Disk Detection"
hijack: removed menu entry: "Serial Port Assignment"
kftpd: listening on port 21
khttpd: listening on port 80
  player.cpp        : 385:empeg-car 2.01 2004/07/06.
Prolux 4 empeg car - 2.1434 Jul  5 2004
Vcb: 0x40577000
! wave_decoder.cpp  : 312:Bytes not (yet) available (0xc0044000)